### Device Usage Page (device_usage_statistics.html)

This HTML page displays the device usage statistics that will be sent to Xilinx. The file also contains predefined XML tags used to simplify processing.
Please verify the contents are okay to send to Xilinx!

Software Version and Target Device
Product Version: | ISE:11.2 (ISE) | Target Family: | spartan3e
OS Platform: | NT | Target Device: | xc3s100e
Project ID (random number) | f925c5ab4edc439c9a978d4fe8167939.b1e9e556a221431f972e48d13fbcbb81.3 | Target Package: | cp132
Registration ID | 174423036 | Target Speed: | -4
Date Generated | Fri 28. Aug 18:59:25 2009

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Registers=2 Flip-Flops=2 | MiscellaneousStatistics AGG_BONDED_IO=4 AGG_IO=4 NUM_BONDED_IBUF=2 NUM_BONDED_IOB=2 NUM_BUFGMUX=1 NUM_IOB_FF=2 | NetStatistics NumNets_Active=7 NumNets_Vcc=1 NumNodesOfType_Active_CLKPIN=2 NumNodesOfType_Active_CNTRLPIN=1 NumNodesOfType_Active_DOUBLE=8 NumNodesOfType_Active_DUMMY=4 NumNodesOfType_Active_DUMMYESC=2 NumNodesOfType_Active_GLOBAL=8 NumNodesOfType_Active_HUNIHEX=2 NumNodesOfType_Active_INPUT=2 NumNodesOfType_Active_IOBOUTPUT=2 NumNodesOfType_Active_OUTPUT=1 NumNodesOfType_Active_VFULLHEX=2 NumNodesOfType_Active_VUNIHEX=1 NumNodesOfType_Vcc_CNTRLPIN=1 NumNodesOfType_Vcc_INPUT=1 NumNodesOfType_Vcc_VCCOUT=2 SiteStatistics IOB-DIFFM=1 IOB-DIFFS=1 | SiteSummary BUFGMUX=1 BUFGMUX_GCLKMUX=1 BUFGMUX_GCLK_BUFFER=1 IBUF=2 IBUF_INBUF=2 IBUF_PAD=2 IOB=2 IOB_OFF1=2 IOB_OUTBUF=2 IOB_PAD=2

Configuration Data
BUFGMUX S=[S_INV:1] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:1] S=[S_INV:1] [S:0] IBUF_PAD IOATTRBOX=[LVCMOS25:2] | IOB O1=[O1_INV:0] [O1:2] OTCLK1=[OTCLK1_INV:0] [OTCLK1:2] SR=[SR:1] [SR_INV:0] IOB_OFF1 CK=[CK:2] [CK_INV:0] D=[D:2] [D_INV:0] LATCH_OR_FF=[FF:2] OFF1_INIT_ATTR=[INIT0:2] OFF1_SR_ATTR=[SRLOW:1] OFFATTRBOX=[SYNC:1] SR=[SR:1] [SR_INV:0] | IOB_OUTBUF IN=[IN_INV:0] [IN:2] IOB_PAD DRIVEATTRBOX=[12:2] IOATTRBOX=[LVCMOS25:2] SLEW=[SLOW:2] |

Pin Data
BUFGMUX I0=1 O=1 S=1 BUFGMUX_GCLKMUX I0=1 OUT=1 S=1 | BUFGMUX_GCLK_BUFFER IN=1 OUT=1 IBUF I=2 PAD=2 IBUF_INBUF IN=2 OUT=2 | IBUF_PAD PAD=2 IOB O1=2 OTCLK1=2 PAD=2 SR=1 IOB_OFF1 CK=2 D=2 Q=2 SR=1 | IOB_OUTBUF IN=2 OUT=2 IOB_PAD PAD=2

Tool Usage
Command Line History xst -ise <ise_file> xst -ise <ise_file> ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf xst -ise <ise_file> ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd fuse

Software Quality
Run Statistics
bitgen | 6 | 6 | 0 | 0 | 0 | 0 | 0
map | 8 | 8 | 0 | 0 | 0 | 0 | 0
ngc2edif | 1 | 1 | 0 | 0 | 0 | 0 | 0
ngdbuild | 9 | 9 | 0 | 0 | 0 | 0 | 0
par | 8 | 8 | 0 | 0 | 0 | 0 | 0
trce | 8 | 8 | 0 | 0 | 0 | 0 | 0
xst | 6 | 6 | 0 | 0 | 0 | 0 | 0

Project Statistics
PROP_Synthesis_Tool=XST (VHDL/Verilog) | PROP_Simulator=ISim (VHDL/Verilog)
PROP_Top_Level_Module_Type=HDL | PROP_PreferredLanguage=Verilog
PROP_Enable_Message_Filtering=false | PROP_Enable_Incremental_Messaging=false
PROP_UseSmartGuide=false | Partitions count=1
FILE_UCF=1 | FILE_VERILOG=2
PROP_DevFamily=Spartan3E | PROP_DevPackage=cp132
PROP_DevSpeed=-4 | PROP_FitterReportFormat=HTML
PROP_Simulator=ISim (VHDL/Verilog) | PROP_UserConstraintEditorPreference=Constraints Editor
PROP_lockPinsUcfFile=changed | Project duration(days)=0

ISim Statistics
Xilinx HDL Libraries Used=
Fuse Resource Usage=370 ms, 57580 KB
Total Signals=12
Total Nets=12
Total Blocks=3
Total Processes=12
Total Simulation Time=1 us
Simulation Resource Usage=0.180259 sec, 251265 KB
Simulation Mode=gui