### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.4 (ISE) - P.49d | Target Family: | Spartan3E
OS Platform: | NT | Target Device: | xc3s100e
Project ID (random number) | b85c5854cbb64ce99b7e2b9e3a74d5ae.7541A142F1754D2DA8C1E4A280B88218.1 | Target Package: | cp132
Registration ID | 205868839_205625405_210133127_560 | Target Speed: | -4
Date Generated | 2013-05-10T11:34:53 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | Service Pack 1 (build 7601)
CPU Name | Intel(R) Core(TM) i7 CPU 975 @ 3.33GHz | CPU Speed | 3340 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Counters=2 25-bit updown counter=1 8-bit updown counter=1 | MiscellaneousStatistics AGG_BONDED_IO=12 AGG_IO=12 AGG_SLICE=39 NUM_4_INPUT_LUT=73 NUM_BONDED_IBUF=4 NUM_BONDED_IOB=8 NUM_BUFGMUX=1 NUM_CYMUX=31 NUM_SLICEL=39 NUM_SLICE_FF=33 NUM_XOR=33 | NetStatistics NumNets_Active=105 NumNets_Vcc=1 NumNodesOfType_Active_CLKPIN=18 NumNodesOfType_Active_CNTRLPIN=36 NumNodesOfType_Active_DOUBLE=137 NumNodesOfType_Active_DUMMY=199 NumNodesOfType_Active_DUMMYESC=4 NumNodesOfType_Active_GLOBAL=11 NumNodesOfType_Active_HUNIHEX=4 NumNodesOfType_Active_INPUT=224 NumNodesOfType_Active_IOBOUTPUT=4 NumNodesOfType_Active_OMUX=83 NumNodesOfType_Active_OUTPUT=89 NumNodesOfType_Active_PREBXBY=46 NumNodesOfType_Active_VFULLHEX=2 NumNodesOfType_Active_VUNIHEX=1 NumNodesOfType_Vcc_CNTRLPIN=1 NumNodesOfType_Vcc_VCCOUT=1 SiteStatistics IBUF-DIFFM=1 IBUF-DIFFMI=1 IOB-DIFFM=2 IOB-DIFFS=5 SLICEL-SLICEM=16 | SiteSummary BUFGMUX=1 BUFGMUX_GCLKMUX=1 BUFGMUX_GCLK_BUFFER=1 IBUF=4 IBUF_INBUF=4 IBUF_PAD=4 IOB=8 IOB_OUTBUF=8 IOB_PAD=8 SLICEL=39 SLICEL_CYMUXF=16 SLICEL_CYMUXG=15 SLICEL_F=39 SLICEL_FFX=17 SLICEL_FFY=16 SLICEL_G=34 SLICEL_XORF=17 SLICEL_XORG=16

Configuration Data
BUFGMUX S=[S_INV:1] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:1] S=[S_INV:1] [S:0] IBUF_PAD IOATTRBOX=[LVCMOS25:4] IOB O1=[O1_INV:0] [O1:8] IOB_OUTBUF IN=[IN_INV:0] [IN:8] IOB_PAD DRIVEATTRBOX=[12:8] IOATTRBOX=[LVCMOS25:8] SLEW=[SLOW:8] | SLICEL BX=[BX_INV:2] [BX:0] CE=[CE:18] [CE_INV:0] CIN=[CIN_INV:0] [CIN:15] CLK=[CLK:18] [CLK_INV:0] SR=[SR:18] [SR_INV:0] SLICEL_CYMUXF 0=[0:16] [0_INV:0] 1=[1_INV:2] [1:14] SLICEL_CYMUXG 0=[0:15] [0_INV:0] | SLICEL_FFX CE=[CE:17] [CE_INV:0] CK=[CK:17] [CK_INV:0] D=[D:17] [D_INV:0] FFX_INIT_ATTR=[INIT0:17] FFX_SR_ATTR=[SRLOW:17] LATCH_OR_FF=[FF:17] SR=[SR:17] [SR_INV:0] SYNC_ATTR=[SYNC:17] | SLICEL_FFY CE=[CE:16] [CE_INV:0] CK=[CK:16] [CK_INV:0] D=[D:16] [D_INV:0] FFY_INIT_ATTR=[INIT0:16] FFY_SR_ATTR=[SRLOW:16] LATCH_OR_FF=[FF:16] SR=[SR:16] [SR_INV:0] SYNC_ATTR=[SYNC:16] | SLICEL_XORF 1=[1_INV:2] [1:15]

Pin Data
BUFGMUX I0=1 O=1 S=1 BUFGMUX_GCLKMUX I0=1 OUT=1 S=1 BUFGMUX_GCLK_BUFFER IN=1 OUT=1 IBUF I=4 PAD=4 IBUF_INBUF IN=4 OUT=4 IBUF_PAD PAD=4 IOB O1=8 PAD=8 IOB_OUTBUF IN=8 OUT=8 | IOB_PAD PAD=8 SLICEL BX=2 CE=18 CIN=15 CLK=18 COUT=15 F1=39 F2=39 F3=22 F4=8 G1=34 G2=34 G3=17 G4=5 SR=18 X=22 XQ=17 Y=18 YQ=16 | SLICEL_CYMUXF 0=16 1=16 OUT=16 S0=16 SLICEL_CYMUXG 0=15 1=15 OUT=15 S0=15 SLICEL_F A1=39 A2=39 A3=22 A4=8 D=39 SLICEL_FFX CE=17 CK=17 D=17 Q=17 SR=17 | SLICEL_FFY CE=16 CK=16 D=16 Q=16 SR=16 SLICEL_G A1=34 A2=34 A3=17 A4=5 D=34 SLICEL_XORF 0=17 1=17 O=17 SLICEL_XORG 0=16 1=16 O=16

Tool Usage
Command Line History xst -ise <ise_file> xst -ise <ise_file> ngdbuild -ise <ise_file> -intstyle ise -dd _ngo -nt timestamp -i -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -v 3 -s 4 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc3s100e-cp132-4 <fname>.ngc <fname>.ngd map -intstyle ise -p xc3s100e-cp132-4 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 4 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
bitgen | 1 | 1 | 0 | 0 | 0 | 0 | 0
compxlib | 3 | 3 | 0 | 0 | 0 | 0 | 0
map | 2 | 2 | 0 | 0 | 0 | 0 | 0
ngdbuild | 3 | 3 | 0 | 0 | 0 | 0 | 0
par | 2 | 2 | 0 | 0 | 0 | 0 | 0
trce | 2 | 2 | 0 | 0 | 0 | 0 | 0
xst | 5 | 5 | 0 | 0 | 0 | 0 | 0

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_LastAppliedGoal=Balanced | PROP_LastAppliedStrategy=Xilinx Default (unlocked)
PROP_ManualCompileOrderImp=false | PROP_PropSpecInProjFile=Store non-default values only
PROP_Simulator=ISim (VHDL/Verilog) | PROP_SynthTopFile=changed
PROP_Top_Level_Module_Type=HDL | PROP_UseSmartGuide=false
PROP_UserConstraintEditorPreference=Text Editor | PROP_intProjectCreationTimestamp=2013-05-10T11:34:07
PROP_intWbtProjectID=7541A142F1754D2DA8C1E4A280B88218 | PROP_intWbtProjectIteration=1
PROP_intWorkingDirLocWRTProjDir=Same | PROP_intWorkingDirUsed=No
PROP_lockPinsUcfFile=changed | PROP_selectedSimRootSourceNode_behav=Module|CountingTheWorld
PROP_AutoTop=true | PROP_DevFamily=Spartan3E
PROP_DevDevice=xc3s100e | PROP_DevFamilyPMName=spartan3e
PROP_DevPackage=cp132 | PROP_Synthesis_Tool=XST (VHDL/Verilog)
PROP_DevSpeed=-4 | PROP_PreferredLanguage=Verilog
FILE_UCF=1 | FILE_VERILOG=1

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FDRE=33 | NGDBUILD_NUM_IBUF=3 | NGDBUILD_NUM_INV=1
NGDBUILD_NUM_LUT2=34 | NGDBUILD_NUM_LUT3=26 | NGDBUILD_NUM_LUT4=10 | NGDBUILD_NUM_LUT4_D=2
NGDBUILD_NUM_LUT4_L=1 | NGDBUILD_NUM_MUXCY=31 | NGDBUILD_NUM_OBUF=8 | NGDBUILD_NUM_XORCY=33
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=1 | NGDBUILD_NUM_FDRE=33 | NGDBUILD_NUM_IBUF=3 | NGDBUILD_NUM_IBUFG=1
NGDBUILD_NUM_INV=1 | NGDBUILD_NUM_LUT2=34 | NGDBUILD_NUM_LUT3=26 | NGDBUILD_NUM_LUT4=10
NGDBUILD_NUM_LUT4_D=2 | NGDBUILD_NUM_LUT4_L=1 | NGDBUILD_NUM_MUXCY=31 | NGDBUILD_NUM_OBUF=8
NGDBUILD_NUM_XORCY=33

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ifmt=mixed | -ofn=<design_top> | -ofmt=NGC
-p=xc3s100e-4-cp132 | -top=<design_top> | -opt_mode=Speed | -opt_level=1
-iuc=NO | -keep_hierarchy=No | -netlist_hierarchy=As_Optimized | -rtlview=Yes
-glob_opt=AllClockNets | -read_cores=YES | -write_timing_constraints=NO | -cross_clock_analysis=NO
-bus_delimiter=<> | -slice_utilization_ratio=100 | -bram_utilization_ratio=100 | -verilog2001=YES
-fsm_extract=YES | -fsm_encoding=Auto | -safe_implementation=No | -fsm_style=LUT
-ram_extract=Yes | -ram_style=Auto | -rom_extract=Yes | -shreg_extract=YES
-rom_style=Auto | -auto_bram_packing=NO | -resource_sharing=YES | -async_to_sync=NO
-mult_style=Auto | -iobuf=YES | -max_fanout=500 | -bufg=24
-register_duplication=YES | -register_balancing=No | -optimize_primitives=NO | -use_clock_enable=Yes
-use_sync_set=Yes | -use_sync_reset=Yes | -iob=Auto | -equivalent_register_removal=YES
-slice_utilization_ratio_maxmargin=5